--list interfaces

WinDump -D

-- listen on interface 3

WinDump -i 3

--listen for icmp traffic

WinDump -i 3 icmp

--listen for traffic between 192.168.1.102 and 192.168.1.104

WinDump -i 3 host 192.168.1.102 and 192.168.1.104

WinDump -i 3 dst port 111

--buffer output (-l), print output in ASCII (-A), most verbose level (-vvv\_, view first 1024 bytes of header (-s 1024)

WinDump -vvvs 1024 -l -A host fir3net.com

-- filter based on src or dest being 1.2.3.4

WinDump -i 3 host 1.2.3.4

--filter based on src 1.2.3.4

WinDump -i 3 src 1.2.3.4

--most verbose

WinDump -i 3 -vvvs 1024 -l -A src 192.168.1.104 and dst port 111

--don't resolve hostnames, non-verbose output

WinDump -i 3 -n

--absolute seqnums

WinDump -i 3 -nS